**Narrow Aisle Forklift Daily Pre-Use Inspection**

|  |  |  |  |
| --- | --- | --- | --- |
| **Make/Model:** | | **Hour Meter:** | |
| **POWER OFF CHECKS** | **Issue?** | **POWER ON CHECKS** | **Issue?** |
| Wheels and Tires |  | Unit starts and runs properly |  |
| Mirrors, visibility aids |  | Instrument/Gauges |  |
| **Battery & Battery compartment** | | Warning lights or audible alarms |  |
| Cables and connectors |  | Horn/other warning devices |  |
| Battery secured |  | No unusual noises |  |
| Vent caps |  | **Forward & Reverse Control** | |
| **Hydraulics** | | Accelerator |  |
| Cylinders/Rods |  | Steering |  |
| Hoses/Lines/Fittings |  | Braking |  |
| Seatbelt/Seat |  | Backup Alarm |  |
| Lifting attachment |  | Parking Brake |  |
| Hood/Covers/Panels |  | Lifting Control |  |
| Grounding strap |  | Emergency quick disconnect |  |
| Oil/Fuel levels |  | Leaks (oil, gas, etc.) |  |

**If there is any issue found during pre-use inspection, notify supervisor immediately and do not use the forklift. Lock out equipment to prevent accidental use by other workers.**

|  |  |  |
| --- | --- | --- |
| **DATE & TIME** | **OPERATOR SIGNATURE** | **COMMENTS** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |